**1 Windows 10 OS**

Include zephyr.

|  |
| --- |
| #include <zephyr/zephyr.h>  #include <zephyr/shell/shell.h> |
| #include <zephyr/bluetooth/audio/audio.h> |

|  |
| --- |
| C:\Users\HP\zephyr  Ru zephyr-env.cmd |

|  |
| --- |
| C:\Users\HP\zephyr\include\ |

Graphical user interface, application, table

Description automatically generated

Graphical user interface, application, table

Description automatically generated

Compiler with zephyr-sdk-0.15.0

|  |
| --- |
| C:\Users\HP\zephyr-sdk-0.15.0\arm-zephyr-eabi\bin\arm-zephyr-eabi-gcc.exe -IC:/Users/HP/zephyr/include |

nrf at C:\Users\HP\nrf\applications

j-link

<https://www.segger.com/downloads/jlink/>

<https://www.nordicsemi.com/Products/Development-tools/nrf-command-line-tools/download>

|  |
| --- |
| nrfjprog -i  nrfjprog --program build/zephyr/zephyr.hex --coprocessor CP\_APPLICATION --chiperase -r |

<https://www.segger.com/products/debug-probes/j-link/tools/rtt-viewer/>

<https://developer.nordicsemi.com/nRF_Connect_SDK/doc/1.3.1/zephyr/guides/tools/nordic_segger.html>